Prestigio DVR RR575W Firmware Update Guide

1. Copy “\*.bin” file from unpacked .zip-archive to the root folder of SD card
2. Power off the device
3. Insert SD card into the device and connect device to the charger
4. Device would power up and update process will start
5. Update process takes approximately 1 min
6. After update process would be finished – delete “\*.bin” file from the SD card.
7. To check FW version put the device into settings mode by the left button, then press and hold the right button until the current version will be shown.