
# Visconte 3 BIOS Update Manual

1. Copy update package folder to the USB disk, run H2OFFT-W.exe as administrator (Right click on the H2OFFT-W.exe and choose to run as Administrator).



1. H2OFFT-W will update BIOS automatically and restart system after finish.

## 